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	Customer Name
	
	Boat Type & Name
	

	Boat Length/Beam
	
	Rig type (top, 7/8,3/4)
	

	Phone
	
	Fax
	

	E-mail
	
	Country, Sail No./Color
	

	If you race your boat, please fill in the measurements based on your current rating certificate or class rules.

	Rule (circle one):  IMS / ORC / IOR / CLASS / other
	


	1
	Main Dimensions
	
	I
	
	J
	

	1.1
	Luff (LF)
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	1.2
	Leech (LL)
	
	

	1.3
	Foot (LF)
	
	

	1.4
	LP (meters or %)
	
	

	
	

	2
	Measurements (if jib’s LP <110%)
	

	2.1
	JH
	
	

	2.2
	JGT
	
	

	2.3
	JGU
	
	

	2.4
	JGM
	
	

	2.5
	JGL
	
	

	
	

	3
	Battens 

(if jib’s LP <110%)
	Length
	Full
	

	3.1
	BL1 (top)
	
	
	

	3.2
	BL2 (upper-mid)
	
	
	

	3.3
	BL3 (lower-mid)
	
	
	

	3.4
	BL4 (bottom)
	
	
	

	3.5
	Parallel Luff
	Y/N
	
	

	
	

	4
	Draft Stripes
	Y/N
	
	

	Color/Quantity
	
	

	
	

	5
	Luff type
	Bolt Rope
	Size
	
	

	
	
	Hanks
	
	

	
	

	6
	Clewboard
	Y/N
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	7
	Mast&Yacht Dimensions
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	7.1
	I
	
	

	7.2
	J
	
	

	7.3
	Max Hoist 
(Forestay Length)
	
	

	7.4
	Mast Section “W”
	
	

	7.5
	Mast Section “T”
	
	

	7.6
	Freeboard at Forestay (FF)
	
	

	7.7
	Freeboard at Mast (FM)
	
	

	7.8
	Stanchion Patches
	1.
	
	

	
	2.
	
	

	
	3.
	
	

	
	

	8
	Spreaders (Lower the tape to the top spreader and measure to the shroud base)
	

	8.1
	Position spreaders over the boom
	Length 
	Angle or Distance
	

	
	1
	
	
	
	

	
	2
	
	
	
	

	
	3
	
	
	
	

	
	4
	
	
	
	

	8.2
	Base point of shrouds
	

	
	Width
	
	

	
	Offset
	
	

	
	Distance to BP
	
	

	
	

	9
	Tracks&Leech
	
	10
	Clew Height Desired
	

	9.1
	Genua
	FWD
	AFT
	
	NOTES:

	
	Leech 
	
	
	
	

	
	Track Position 
	
	
	
	

	
	Track Offset
	
	
	
	

	9.2
	Jib
	FWD
	AFT
	
	

	
	Leech 
	
	
	
	

	
	Track Position 
	
	
	
	

	
	Track Offset
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	13
	Furling System
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	13.1
	Manufacturer
	
	

	13.2
	Model #
	
	

	13.3
	Foil Tape Size
	
	

	13.4
	OE#
	
	

	
	

	14
	Furling Details
	

	14.1
	Forestay Length
	
	

	14.2
	Forestay Distance
	
	

	14.3
	Max Luff Length
	
	

	14.4
	Feeder Height
	
	

	14.5
	Drum Height
	
	

	14.6
	Tack Setback
	
	

	14.7
	Drum
	
	

	
	

	15
	U.V. Cover
	

	15.1
	Material
	
	

	15.2
	Color
	
	

	15.3
	Port or Starbord
	
	

	

	16
	Forestay Tension
	HIGH (small sag)
	
	MEDIUM sag
	
	LOW (big sag)
	

	

	17
	Forestay Tensioned by
	Turnbuckle
	
	Mechanical
	
	Runners
	

	
	Purchase
	
	Hydraulic
	
	
	

	

	NOTES:



